# This is a udev config file to grant 0666 (world readable/writable) for all
# hid devices on Linux systems.


# If you are using the libusb implementation of hidapi (hid-libusb.c), then
# use something like the following line, adding the VID and PID with
# those of your device. Note that for kernels before 2.6.24, you will need
# to substitute "usb" with "usb_device". It shouldn't hurt to use two lines
# (one each way) for compatibility with older systems.

# HIDAPI/libusb
SUBSYSTEM=="usb", MODE="0666"


# If you are using the hidraw implementation, then do something like the
# following, adding the VID and PID with your device. Busnum 1 is USB.

# HIDAPI/hidraw
KERNEL=="hidraw*", MODE="0666"

# Once done, optionally rename this file for your device, and drop it into
# /etc/udev/rules.d and unplug and re-plug your device. This is all that is
# necessary to see the new permissions. Udev does not have to be restarted.

# Note that the hexadecimal values for VID and PID are case sensitive and
# must be lower case.

# If you think permissions of 0666 are too loose, then see:
# http://reactivated.net/writing_udev_rules.html for more information on finer
# grained permission setting. For example, it might be sufficient to just
# set the group or user owner for specific devices (for example the plugdev
# group on some systems).
